### Cleaning the paper pick-up roller

1 | Turn off the printer power switch and then unplug the printer.
2 | Pull the paper tray completely out of the printer.
3 | Tightly wring out a lint-free cloth soaked in lukewarm water, and then wipe the separator pad (1) of the paper tray with it to remove dust.
4 | Wipe the two pick-up rollers (1) inside of the printer to remove dust.
5 | Put the paper tray back in the printer.
6 | Plug the printer back in, and then turn on the power switch.

Page Top