### Belt unit

Model Name: BU-200CL
A new belt unit can print approximately 50,000 A4 or Letter size single-sided pages.

#### Belt End Soon message

Belt End Soon

If the LCD shows Belt End Soon, it means the belt unit is near the end of its life. Buy a new belt unit and have it ready before you get a Replace Belt message. To replace the belt unit, see Replacing the belt unit.
Page Top

#### Replace Belt message

When the following message appears on the LCD, you need to replace the belt unit:

Replace Belt

IMPORTANT

• | DO NOT touch the surface of the belt unit. If you touch it, it could degrade print quality.
• | Damage caused by incorrect handling of the belt unit may void your warranty.

Page Top

#### Replacing the belt unit

1 | Turn off the printer power switch. Fully open the top cover by lifting up on the handle (1).
2 | Take out all the drum unit and toner cartridge assemblies. IMPORTANT
• | We recommend that you place the drum unit and toner cartridge assembly on a clean, flat surface with a sheet of disposable paper or cloth underneath it in case you accidentally spill or scatter toner.
• | To prevent damage to the printer from static electricity, DO NOT touch the electrodes shown in the illustration.
• | Handle the toner cartridge carefully. If toner scatters on your hands or clothes, wipe or wash it off with cold water at once.
• | To avoid print quality problems, DO NOT touch the shaded parts shown in the illustrations.
3 | Hold the green handle of the belt unit and lift the belt unit up, then pull it out. IMPORTANT
| To avoid print quality problems, DO NOT touch the shaded parts shown in the illustrations.
4 | Unpack the new belt unit and put the new belt unit in the printer.
5 | Slide each drum unit and toner cartridge assembly into the printer. Make sure that you match the toner cartridge colour to the same colour label on the printer. Repeat this for all the drum unit and toner cartridge assemblies.
C - Cyan M - Magenta | Y - Yellow K - Black
6 | Close the top cover of the printer.

When you replace the belt unit with a new one, you need to reset the belt unit counter by completing the following steps:

1 | Turn the printer power switch back on.
2 | Press + or - to choose Machine Info..
3 | Press OK to proceed to the next menu level, and then press + or - to choose Reset Parts Life.
4 | Press OK, and then press + to choose Belt Unit.
5 | Press OK two times.

Page Top