## Cleaning

Clean the outside and inside of the printer regularly with a dry, lint-free cloth. When you replace the toner cartridge or the drum unit, make sure that you clean the inside of the printer. If printed pages are stained with toner, clean the inside of the printer with a dry, lint-free cloth.
WARNING

| Use neutral detergents. Cleaning with volatile liquids such as thinner or benzine will damage the surface of the printer.
| DO NOT use cleaning materials that contain ammonia.
| DO NOT use flammable substances, any type of spray or any organic solvent/liquids containing alcohol or ammonia to clean the inside or outside of the printer.
| Be careful not to inhale toner.

### Cleaning the outside of the printer

1 | Turn off the printer power switch and then unplug the printer.
2 | Pull the paper tray completely out of the printer.
3 | Wipe the outside of the printer with a dry, lint-free cloth to remove dust.
4 | Remove anything that is stuck inside the paper tray.
5 | Wipe the inside of the paper tray with a dry, lint-free cloth to remove dust.
6 | Put the paper tray back in the printer.
7 | Plug the printer back in, and then turn on the power switch.

Page Top