|  |  |  |  |
| --- | --- | --- | --- |
| **COOLING CHANNEL EQUIPMENT** | **QUANTITY** | **WEIGHT       (kg)** | **TOTAL WEIGHT** |
| **RACK FRAME** | **1** | **70.00** | **70.00** |
| **RACK DOOR (Front/Back)** | **2** | **22.00** | **44.00** |
| **RACK SIDE PANELS** | **2** | **20.00** | **40.00** |

The total weight of the iron in the rack itself will be **158Kg**

This includes the idea that a door will need to be fitted to the front of the racks to give a closed box.